{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":100,"n_cols":2,"rows_kept":100,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["無題1 - マルチファンクションアナライザ 報告書作成手順書エディタ"]
[]
["3 - 1"]
[null,"JTAG:"]
[null,"ARM940  IR:total(4), position(0)  BYPASS: total(1), position(0)"]
[]
[null,"Date: 2012/09/19 13:41:55"]
[]
["8 - 1"]
{"$rows_empty":24}
[null,"Date: 2012/09/19 13:41:59"]
[null,"Mode: Acquisition = Realtime-sampling Persitence = Single"]
[null,"VerticalSettings CH1: Attenuation = x 10 V Range = 1.0v/div Couping = DC Band = Full"]
[null,"Trigger: Mode = Normal Source = CH1 Rising-Edge"]
[null,"Trigger Other Settins: Trigger Lv. CH1 = 1.50v"]
[null,"Horizontal Settings: H Range = 250us/div Sampling = 1,000,000 S/s (5.00 us/pt)"]
[null,"Horizontal Position: Trigger = 49.97 %"]
[]
["11 - 1"]
[null,"機能: 直流電圧計"]
[null,"電圧レンジ: 40v"]
[null,"電圧値: +5.00v"]
[null,"日時: 2012/09/19 13:42:01"]
[]
["11 - 2"]
[null,"機能: 直流電圧計"]
[null,"電圧レンジ: 40v"]
[null,"電圧値: +5.00v"]
[null,"日時: 2012/09/19 14:12:01"]
[]
["11 - 3"]
[null,"機能: 直流電圧計"]
[null,"電圧レンジ: 40v"]
[null,"電圧値: +5.00v"]
[null,"日時: 2012/09/19 14:42:01"]
[]
["11 - 4"]
[null,"機能: 直流電圧計"]
[null,"電圧レンジ: 40v"]
[null,"電圧値: +5.00v"]
[null,"日時: 2012/09/19 15:12:01"]
[]
["11 - 5"]
[null,"機能: 直流電圧計"]
[null,"電圧レンジ: 40v"]
[null,"電圧値: +5.00v"]
[null,"日時: 2012/09/19 15:42:01"]
[]
["11 - 6"]
[null,"機能: 直流電圧計"]
[null,"電圧レンジ: 40v"]
[null,"電圧値: +5.00v"]
[null,"日時: 2012/09/19 16:12:01"]
[]
["11 - 7"]
[null,"機能: 直流電圧計"]
[null,"電圧レンジ: 40v"]
[null,"電圧値: +5.00v"]
[null,"日時: 2012/09/19 16:42:01"]
[]
["11 - 8"]
[null,"機能: 直流電圧計"]
[null,"電圧レンジ: 40v"]
[null,"電圧値: +5.00v"]
[null,"日時: 2012/09/19 17:12:01"]
[]
["11 - 9"]
[null,"機能: 直流電圧計"]
[null,"電圧レンジ: 40v"]
[null,"電圧値: +5.00v"]
[null,"日時: 2012/09/19 17:42:01"]
[]
["11 - 10"]
[null,"機能: 直流電圧計"]
[null,"電圧レンジ: 40v"]
[null,"電圧値: +5.00v"]
[null,"日時: 2012/09/19 18:12:01"]